
# LM386 Amplifier

LM386 is power amplifier IC designed for use in low voltage consumer applications. It is used in various field of electronics applications like Radio amplifier, TV sound systems, power converter etc. The gain of the IC can be varied from 20 to 200 using external circuit or components.


## Usage/Examples

Wien bridge oscillator

Power converters

Ultrasonic drivers

Small servo drivers

Intercoms

Line drivers

TV sound systems

Portable tape player amplifiers

AM to FM radio amplifiers

Audio boosters

Used in speakers of laptop & portable

Used for voice record from microphone, battery operated speakers.


## Documentation

To know the details of LM386 IC please go through with the documentation : [LM386_datasheet](https://www.ti.com/lit/ds/symlink/lm386.pdf)

## Comments/Notes

Please note this is a complete analog IC. It works fine at the time of simulation. But remember there may be minor error for very high gain.

## Contributer

Name: Ankush Mondal
Email: mondalankush369@gmail.com
Year: 2022
Position: FOSSEE Summer Fellow 2022