
# CD4023 IC

It is 3-input NAND Gate IC. CD4023 IC is designed with 180nm CMOS technology in eSim consisting three NAND Gates. When both the inputs are HIGH then only output is LOW, otherwise HIGH. It is also called inverted AND Gate, a type of Universal logic Gate.


## Usage/Examples

Burglar alarm

Freezer warning buzzer

## Documentation

To know the details of CD4023 IC please go through with the documentation : [CD4023_datasheet](https://www.ti.com/lit/gpn/cd4023b)

## Comments/Notes

Please note this is a complete digital IC. It works fine at the time of simulation.

## Contributer

Name: Ankush Mondal
Email: mondalankush369@gmail.com
Year: 2022
Position: FOSSEE Summer Fellow 2022