
# CD4077 IC

It is 2-input XNOR Gate IC. CD4077 IC is designed with 180nm CMOS technology in eSim consisting four XNOR Gates. It plays the role of even 1’s detector. When both inputs are same, then output is HIGH, else LOW. It is also known as Special logic Gate.

## Usage/Examples

Logical Comparators

Adders, Subtractors

Parity Generators and Checkers

Touch sensor circuit
## Documentation

To know the details of CD4077 IC please go through with the documentation : [CD4077_datasheet](https://www.ti.com/lit/gpn/cd4077b)

## Comments/Notes

Please note this is a complete digital IC. It works fine at the time of simulation.

## Contributer

Name: Ankush Mondal
Email: mondalankush369@gmail.com
Year: 2022
Position: FOSSEE Summer Fellow 2022