
# CD4011 IC

It is 2-input NAND Gate IC. CD4011 IC is designed with 180nm CMOS technology in eSim consisting four NAND Gates. When both the inputs are HIGH then only output is LOW, otherwise HIGH. It is also called inverted AND Gate, a type of Universal Gate.


## Usage/Examples

Employed in portable Audio Docks

Used in AV Receivers

Used in MP3 Players or Recorders

Applied in Home Theater

Incorporated in Blu-Ray Players

## Documentation

To know the details of CD4011 IC please go through with the documentation : [CD4011_datasheet](https://www.ti.com/lit/gpn/cd4011b)

## Comments/Notes

Please note this is a complete digital IC. It works fine at the time of simulation.

## Contributer

Name: Ankush Mondal
Email: mondalankush369@gmail.com
Year: 2022
Position: FOSSEE Summer Fellow 2022