
# LM393 Comparator IC

LM393 is a Low power, low offset voltage comparator IC. It has two channels sharing common biasing. It is a high precision comparator with a low offset voltage of 2 mV. It has various applications such as in limit comparators, A/D convertors, wave shaping circuits etc.


## Usage/Examples

Basic Comparator  

CMOS/TTL Driver

Pulse Train Generator

Crystal Controlled Oscillator

Positive/Negative Floating Regulator

Two-Decade High Frequency VCO


## Documentation

To know the details of LM393 IC please refer to this link [LM393_datasheet.](https://www.ti.com/lit/ds/symlink/lm393-n.pdf?ts=1665939843518&ref_url=https%253A%252F%252Fwww.google.com%252F)

## Comments/Notes

Please note this is a complete analog IC. It works fine at the time of simulation.

## Contributor

Name: Arpit Sharma  
Email: arpitniraliya306@gmail.com  
Year: 2022  
Position: FOSSEE Summer Fellowship Intern 2022
