
# LM1458 Dual Operational Amplifier IC

LM1458 is a general purpose, Dual Channel Operational Amplifier IC. Both the Amplifiers operate independently but they share common supply. It has inbuilt short circuit protection & offers low power consumption. No frequency compensation is needed.


## Usage/Examples

Inverting/Non-Inverting Amplifier

Integrator/Summer

Differential Amplifier

Differentiator

Schmitt Trigger

Comparators


## Documentation

To know the details of LM1458 IC please refer to this link [LM1458_datasheet.](https://www.ti.com/lit/ds/symlink/lm1458.pdf?ts=1665941946373&ref_url=https%253A%252F%252Fwww.google.com%252F)

## Comments/Notes

Please note this is a complete analog IC. It works fine at the time of simulation.

## Contributor

Name: Arpit Sharma  
Email: arpitniraliya306@gmail.com  
Year: 2022  
Position: FOSSEE Summer Fellowship Intern 2022
