
# CD4028 IC

It is BCD to Decimal converter IC. CD4028 IC is designed with 180nm CMOS technology in eSim. It is 16 pin IC. 
## Usage/Examples

Code Conversion

Indication-Tube Decoder

Address Decoding

Memory Selection Control
## Documentation

To know the details of CD4028 IC please go through with the documentation : [CD4028_datasheet](https://www.ti.com/lit/gpn/cd4028b)

## Comments/Notes

Please note this is a complete digital IC. It works fine at the time of simulation.

## Contributer

Name: Ankush Mondal
Email: mondalankush369@gmail.com
Year: 2022
Position: FOSSEE Summer Fellow 2022