|  |  |  |  |
| --- | --- | --- | --- |
|  | Name | Description | Quantity |
|  | R1 | 100 ohm Resistor (Br-Bl-Br) | 1 |
|  | R2, R3, R4 | 91 ohm Resistor (Wt-Br-Bl) | 3 |
|  | R5, R6, R7, R8 | 10K ohm Resistor (Br-Bl-Or) | 4 |
|  | R9 | 1K ohm Resistor (Br-Bl-Rd) | 1 |
|  | D1 | Diode | 1 |
|  | Relay | Relay | 1 |
|  | X1 | Terminal Block | 1 |
|  | Piezo | Piezo | 1 |
|  | LED1 | LED - 2 lead | 1 |
|  | LED2 | RGB LED | 1 |
|  | T1 | Transistor | 1 |
|  | SWITCH | Switch | 1 |
|  | BUTTON, RESET | Push Button | 2 |
|  | PHOTO | Photo Resistor | 1 |
|  | HALL | Hall effect sensor | 1 |
|  | POT | Potentiometer | 1 |
|  | ENC | Rotary encoder | 1 |
|  | THERM | Thermistor | 1 |
|  | SERVO | Servo | 1 |
|  | SERVO-PARTS | Servo parts | 1 |
|  | NUT, BOLT | Nut & Bolt | 2 |
|  | HEADER | 6x Pin header | 2 |
|  | HEADER | 8x Pin header | 2 |